|  |
| --- |
| Surface Type: RoofsBMP L603: Downspout Dispersion (Dispersion Trenches and Splashblocks) City of Tacoma Permit Number: Click here to enter text.Date Prepared: Click here to enter a date. |
|  |
|  | ***Yes*** | ***No*** | ***NA*** |
| Can the dispersion trench or splashblock be placed 10 feet or more from any building structure? |[ ] [ ] [ ]
| Can the dispersion trench or splashblock be placed 5 feet or more from any other structure or property line? |[ ] [ ] [ ]
| Can the dispersion trench or splashblock be placed 50 feet or more from the top of a steep slope (15% or greater)?  |[ ] [ ] [ ]
| Is it possible to maintain or construct a vegetated flowpath of at least 25 feet from the outlet of a dispersion trench and any property line, structure, stream, wetland, other infiltration or dispersion system, or impervious surface? |[ ] [ ] [ ]
| Is it possible to maintain or construct a vegetated flowpath of at least 50 feet from the outlet of a dispersion trench and any slope greater than 15%?  |[ ] [ ] [ ]
| Is it possible to maintain or construct a vegetated flowpath of at least 50 feet from the outlet of splashblock and any property line, structure, stream, wetland, other infiltration or dispersion system, or impervious surface? |[ ] [ ] [ ]
| Will installing a dispersion trench or splashblocks cause conflicts with any of the following? (An answer of yes means this BMP is not feasible). |[ ] [ ] [ ]
| ***Please check the box next to those items that apply.* Answer requires a report prepared by professional.** |
| Requirements of the Historic Preservation Laws and Archeology Laws, Federal Superfund or Washington State Model Toxics Control Act, Federal Aviation Administration requirements for airports, or Americans with Disability Act |[ ]
| Special zoning district design criteria adopted and being implemented through any City of Tacoma planning efforts |[ ]
| Public health and safety standards |[ ]
| Transportation regulations to maintain the option for future expansion or multi-modal use of public rights-of-way |[ ]
| Critical Area Preservation Ordinance  |[ ]