|  |
| --- |
| Surface Type: Roofs and Other Hard SurfacesBMP L614: Full Dispersion City of Tacoma Permit Number: Click here to enter text.Date Prepared: Click here to enter a date. |
|  |
|  | ***Yes*** | ***No*** | ***NA*** |
| For residential projects, is the ratio of the native vegetation area to the impervious area greater than 65% to 10%?  |[ ] [x] [ ]
| For projects other than residential projects, has the proposed project retained 65% or greater of the native vegetation on the project site? |[ ] [x] [ ]
| Is it possible to maintain a native vegetated flowpath of at least 100 feet from the discharge point of a hard surface to any property line, structure, stream, wetland, other infiltration or dispersion system, or impervious surface?  |[ ] [x] [ ]
| Is it possible to maintain a native vegetated flowpath of at least 25 feet from the discharge from cleared areas (non-native landscaping, lawn, and/or pasture) to any property line, structure, stream, wetland, other infiltration or dispersion system, or impervious surface? |[ ] [x] [ ]